Job:

# Cold Water Start

## For Hi Delta® Models 992C-2342C


Engineer:

Contractor:

Prepared By:       Date:

Model:       Indoor/Outdoor:       MBTUH Input:

* Approved for hydronic systems ONLY



* 100% Factory Fire Tested System
* PID Control Logic
* Fail-Safe Operation
* Spring-Return Actuator
* Adjustable Inlet Temperature (105° - 120°F)
* Microprocessor Start-up Sequence

Hi Delta Boiler

* In-line Pump Available for Models 1262C–­2342C;   
  Integral Pump Available for Model 992C Only  
   \*Pump selection based on 75 equivalent feet of piping equal to connection size.





Proudly Made in the USA

**Inline Pump**

**Models 1262C – 2342C**








#### Cold Water Start

#### For Hi Delta 992C-2342C Model

**Integral Pump  
Models 992C Only**



See also these submittals:   
Hi Delta Models H 992C-2342C – Catalog No. 2000.312

Delta Ltd Models H 989B-2339B Catalog No. 2000.471

Raypak, Inc. ▪ 2151 Eastman Avenue, Oxnard, CA 93030 ▪ (805) 278-5300 ▪ Fax (800) 872-9725 ▪ www.raypak.com