­­Job:

# Stainless Steel 110-Gallon Non-ASME Storage Tank

##

Engineer:

Contractor:

Prepared By:       Date:

Model:

* 444 Stainless Steel Construction
* Fully Seam-Welded Construction
	+ No Lining to Fail
* Fully Pickled and Passivated for Maximum Durability
* 100% Pressure Tested Tank and Coil
* R-18 – 3-1/4 Inch Thick High-Density Neopor® GPS Insulation
	+ Graphite Impregnated for Superior Performance
* Indoor – Outdoor Installation
* UV Stable Polypropylene Jacket
* UV Stable EPS Caps Top and Bottom
* 150 PSI Max Pressure Rating
* 180 ͦF Maximum Tank Temperature
* 2 Inch NPT Water Connections
* Hand-Hole Inspection and Cleanout Port
* Sensor / Tankstat Drywell Standard
* No Anodes or Dielectric Fittings Required
* All Tank Connections are on the Side for Easy Installation in Low-Clearance Areas
* Commercial 5-Year Warranty

Stainless Steel Indirect Fired Storage Water Heater

Model Number



|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Model** | **Shipping****Weight****Lb. (kg)** | **Operating****Weight****Lb. (kg)** | **Water****Inlet/****Outlet** | **Diameter****In./(mm)****(A)** | **Height****In./(mm)****(B)** | **To Heater****Height****In./(mm)****(C)** | **Water****Outlet/T&P****Height****In./(mm)****(D)** | **From Heater****Height****In./(mm)****(E)** | **Drywell****Height****In./(mm)****(F)** |
| RSST110 | 150(68) | 1100 (500) | 2 NPT | 31.3 (795) | 67.3 (1710) | 12.2 (310) | 54.8(1392) | 22 (558) | 27.9 (708) |

Raypak, Inc. ▪ 2151 Eastman Ave., Oxnard, CA 93030 ▪ (805) 278-5300 ▪ Fax (800) 872-9725 ▪ www.raypak.com